**Aqueduct Flood Hazard**

5



|  |  |  |  |
| --- | --- | --- | --- |
| Dataset Code: aqueductFloodHazard | | | |
| Aqueduct 3.0 introduces an updated water risk framework and new and improved indicators. It also features different hydrological sub-basins. The indicators based on a new hydrological model that now features (1) integrated water supply and demand, (2) surface water and groundwater modeling, (3) higher spatial resolution, and (4) a monthly time series that enables the provision of monthly scores for selected indicators. | | | |
| **Citation:**  Hofste, R., Kuzma, S., Walker, S., Sutanudjaja, E., Bierkens, M., Kuijper, M., Faneca Sanchez, M., Van Beek, R., Wada, Y., Galvis Rodríguez, S., Reig, P. (2019). Aqueduct 3.0: Updated Decision-Relevant Global Water Risk Indicators. World Resources Institute, July, 1–53. https://doi.org/10.46830/writn.18.00146 | | | |
| **Layers:**  2-year flood, 5-year flood, 10-year flood, 25-year flood, 50-year flood, 100-year flood, 250-year flood, 500-year flood, 1000-year flood | | | |
| **Year/s:**  2020 | **Format:**  .tif | **Resolution:**  PCR-GLOBWB 2 using 5 × 5 arc minute spatial resolution | **Units:**  Numeric |
| **Source Link:**  https://www.wri.org/data/aqueduct-floods-hazard-maps | | | |
|  | | | |